	GHPs ARE NOT ENERGY EFFICIENT

	    FALSEGHPs offer heating and/or water heating efficiencies around 140% and save consumers money over conventional gas or electric systems.


	

	GHPs CAN’T BE INTEGRATED WITH BOILERS, WATER HEATERS, CHILLERS, AND OTHER EQUIPMENT

	    FALSE As hydronic equipment, GHPs are easily integrated into existing systems to support both space and water heating. Some GHPs even offer heat recovery for water heating during cooling season.



	

	GHPs ARE DIFFICULT AND EXTREMELY EXPENSIVE TO MAINTAIN

	    FALSEEngine-driven heat pumps have similar maintenance requirements to electric heat pumps with the addition of maintenance on the engine itself. Absorption GHPs require simple annual maintenance that often costs less than servicing a condensing boiler. Components requiring service include the burner, fan, and fin coils. 



	

	HEAT PUMPS ARE ONLY SUITABLE FOR INSTALLATION IN WARM CLIMATES

	    FALSEGHPs perform well in both warm climates and cold climates, with ratings to perform below 0⁰F without significant capacity reduction. Offering the advantage of a gas burner, GHPs can act like a condensing boiler in sub-zero temperatures maintaining optimal efficiencies for space and water heating with no backup required. In reality, electric heat pumps are more often installed in warmer climates. 





	

	GHPs ARE LOUD

	    FALSEMost absorption and engine-driven GHPs operate at a low noise level which is typically less than 65 db. To compare, a vacuum cleaner operates between 70-80 db.



	

	GHPs OFFER A SHORT LIFESPAN

	     FALSEAbsorption GHPs typically last well over 20 years. An engine-driven GHP has an expected lifespan of 14 years that can extend to 20 years with proper maintenance. 



	

	THERE ARE FEW OPTIONS FOR GHPs

	     FALSEDepending on existing infrastructure, GHPs are available in air-to-air, hydronic, or geothermal systems. Many offer a modular design feature with the option to scale and expand if needed, and indoor units are available with options similar to electric heat pumps. Variable Refrigerant Flow (VRF) type GHPs are capable of providing simultaneous cooling and heating function. 
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FOR MORE INFORMATION VISIT: WWW.GASHEATPUMPS.COM
[image: ]

FOR MORE INFORMATION VISIT: WWW.GASHEATPUMPS.COM
[image: ]

image7.png




image8.emf
© Energy Solutions Center Inc. — All Rights Reserved










image9.emf
© Energy Solutions Center Inc. — All Rights Reserved










image10.png




image1.png




image2.png




image3.png




image4.png




image5.png




image6.png




